Instructions for using KF163X.EXE to produce upto 32 channel EPROM image
for the CDP18U42CD Eprom as used in the Bosch KF163 DigX version. 

It is based on the S89 prescaler which uses a divide ratio of 100/101 and a
reference frequency of 12.5kHz for 12.5 & 25kHz channelled radios.  

Its a DOS based program and can be run from the command prompt in Windows.

KF163X.PRG is an ASCII text file. Each line contains:-

<Channel Number> <Rx Frequency> <Tx Frequency>

eg:-

01 1455000 1455000
02 1456125 1450125


KF163X.EXE scans this file and produces KF163X.BIN, a binary image of the 
CDP18U42CD EPROM for a 12.5kHz reference frequency ONLY. Receive data is 
stored in addresses 00 to 7F (0 to 127) and the Transmit data is stored in 
addresses 80 to FF (128 to 255), four addresses for each channel.

For the 10kHz reference frequency models, please use KF163X10.exe found in 
the KF163X10.ZIP archive

An example KF163X.PRG and its .BIN file are included.  Use DEBUG.EXE to view
the binary file, i.e "DEBUG KF163X.BIN" then "d" to dump twice and then "q" 
to quit DEBUG, again using the commamd prompt.

Any feedback would be welcome.

The program was written by Richard Newton, 2nd March 2006.
(g0ewh@yahoo.co.uk)  


Istruzioni per l'uso KF163X.EXE per produrre 32 immagini EPROM canale fino a
per il CDP18U42CD Eprom come usato nella versione Bosch KF163 DigX .

Si basa sul prescaler S89 che utilizza un rapporto di divisione di 100/101 e
frequenza di riferimento di 12,5 kHz a 12,5 e 25kHz incanalata radio .

Il suo un programma basato su DOS e può essere eseguito dal prompt dei comandi in Windows .

KF163X.PRG è un file di testo ASCII . Ogni riga contiene : -

<numero_canale> RX> Frequency> <TX Frequency>

ad esempio : -

01 1455000 1455000
02 1456125 1450125


KF163X.EXE analizza il file e produce KF163X.BIN , l'immagine binaria del
CDP18U42CD EPROM per una frequenza di riferimento 12.5kHz SOLTANTO. Ricezione dati
memorizzati in indirizzi 00 a 7F ( da 0 a 127 ) ei dati di trasmissione verrà memorizzata nella
indirizzi 80 a FF (128 255) , quattro indirizzi per ciascun canale .

Per i modelli di riferimento di frequenza 10kHz , si prega di utilizzare KF163X10.exe trovato in
l'archivio KF163X10.ZIP

Un esempio KF163X.PRG e il file . BIN sono inclusi. Utilizzare DEBUG.EXE per visualizzare
il file binario , vale a dire " DEBUG KF163X.BIN " poi " d " per scaricare due volte e quindi " q "
per uscire DEBUG , sempre utilizzando il prompt commamd .




